From 72ff51d8dd262d1fef25baedc2ac35116435be47 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Petr=20=C5=A0tetiar?= <ynezz@true.cz>
Date: Wed, 6 Mar 2019 17:54:03 +0100
Subject: [PATCH] serial: ar933x_uart: Fix build failure with disabled console
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Andrey has reported on OpenWrt's bug tracking system[1], that he
currently can't use ar93xx_uart as pure serial UART without console
(CONFIG_SERIAL_8250_CONSOLE and CONFIG_SERIAL_AR933X_CONSOLE undefined),
because compilation ends with following error:

 ar933x_uart.c: In function 'ar933x_uart_console_write':
 ar933x_uart.c:550:14: error: 'struct uart_port' has no
                               member named 'sysrq'

So this patch moves all the code related to console handling behind
series of CONFIG_SERIAL_AR933X_CONSOLE ifdefs.

1. https://bugs.openwrt.org/index.php?do=details&task_id=2152

Cc: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Cc: Jiri Slaby <jslaby@suse.com>
Cc: Andrey Batyiev <batyiev@gmail.com>
Reported-by: Andrey Batyiev <batyiev@gmail.com>
Tested-by: Andrey Batyiev <batyiev@gmail.com>
Signed-off-by: Petr Štetiar <ynezz@true.cz>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/tty/serial/ar933x_uart.c | 24 ++++++++----------------
 1 file changed, 8 insertions(+), 16 deletions(-)

--- a/drivers/tty/serial/ar933x_uart.c
+++ b/drivers/tty/serial/ar933x_uart.c
@@ -52,11 +52,6 @@ struct ar933x_uart_port {
 	struct clk		*clk;
 };
 
-static inline bool ar933x_uart_console_enabled(void)
-{
-	return IS_ENABLED(CONFIG_SERIAL_AR933X_CONSOLE);
-}
-
 static inline unsigned int ar933x_uart_read(struct ar933x_uart_port *up,
 					    int offset)
 {
@@ -511,6 +506,7 @@ static const struct uart_ops ar933x_uart
 	.verify_port	= ar933x_uart_verify_port,
 };
 
+#ifdef CONFIG_SERIAL_AR933X_CONSOLE
 static struct ar933x_uart_port *
 ar933x_console_ports[CONFIG_SERIAL_AR933X_NR_UARTS];
 
@@ -607,14 +603,7 @@ static struct console ar933x_uart_consol
 	.index		= -1,
 	.data		= &ar933x_uart_driver,
 };
-
-static void ar933x_uart_add_console_port(struct ar933x_uart_port *up)
-{
-	if (!ar933x_uart_console_enabled())
-		return;
-
-	ar933x_console_ports[up->port.line] = up;
-}
+#endif /* CONFIG_SERIAL_AR933X_CONSOLE */
 
 static struct uart_driver ar933x_uart_driver = {
 	.owner		= THIS_MODULE,
@@ -703,7 +692,9 @@ static int ar933x_uart_probe(struct plat
 	baud = ar933x_uart_get_baud(port->uartclk, 0, AR933X_UART_MAX_STEP);
 	up->max_baud = min_t(unsigned int, baud, AR933X_UART_MAX_BAUD);
 
-	ar933x_uart_add_console_port(up);
+#ifdef CONFIG_SERIAL_AR933X_CONSOLE
+	ar933x_console_ports[up->port.line] = up;
+#endif
 
 	ret = uart_add_one_port(&ar933x_uart_driver, &up->port);
 	if (ret)
@@ -752,8 +743,9 @@ static int __init ar933x_uart_init(void)
 {
 	int ret;
 
-	if (ar933x_uart_console_enabled())
-		ar933x_uart_driver.cons = &ar933x_uart_console;
+#ifdef CONFIG_SERIAL_AR933X_CONSOLE
+	ar933x_uart_driver.cons = &ar933x_uart_console;
+#endif
 
 	ret = uart_register_driver(&ar933x_uart_driver);
 	if (ret)
