--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -1061,6 +1061,11 @@ static const struct flash_info spi_nor_i
 			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
 			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
 	},
+	{
+		"gd25q512", INFO(0xc84020, 0, 64 * 1024, 1024,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB | SPI_NOR_4B_OPCODES)
+	},
 
 	/* Intel/Numonyx -- xxxs33b */
 	{ "160s33b",  INFO(0x898911, 0, 64 * 1024,  32, 0) },
