From da89f500cb55fb3f19c4b399b46d8add0abbd4d6 Mon Sep 17 00:00:00 2001
From: Mathias Kresin <dev@kresin.me>
Date: Wed, 25 Jul 2018 10:37:48 +0200
Subject: [PATCH] ARM: dts: qcom: ipq4019: fix PCI range

The PCI range is invalid and PCI attached devices doen't work.

Signed-off-by: Mathias Kresin <dev@kresin.me>
Signed-off-by: John Crispin <john@phrozen.org>
Signed-off-by: Andy Gross <andy.gross@linaro.org>
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -401,7 +401,7 @@
 			#size-cells = <2>;
 
 			ranges = <0x81000000 0 0x40200000 0x40200000 0 0x00100000
-				  0x82000000 0 0x48000000 0x48000000 0 0x10000000>;
+				  0x82000000 0 0x40300000 0x40300000 0 0x400000>;
 
 			interrupts = <GIC_SPI 141 IRQ_TYPE_EDGE_RISING>;
 			interrupt-names = "msi";
