From 4a228ecf553e879bae384e634bb6413438e81a0e Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Mon, 11 Mar 2019 15:43:05 +0100
Subject: [PATCH 1/2] ARM: dts: gemini: Indent DIR-685 partition table

It is discouraged to have OF partitions as subnodes directly
under the device, create a "partitions" subnode and put the
partitions inside it.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 arch/arm/boot/dts/gemini-dlink-dir-685.dts | 82 ++++++++++++----------
 1 file changed, 44 insertions(+), 38 deletions(-)

diff --git a/arch/arm/boot/dts/gemini-dlink-dir-685.dts b/arch/arm/boot/dts/gemini-dlink-dir-685.dts
index 9b2824816ddc..50ff65d95f26 100644
--- a/arch/arm/boot/dts/gemini-dlink-dir-685.dts
+++ b/arch/arm/boot/dts/gemini-dlink-dir-685.dts
@@ -267,44 +267,50 @@
 			/* 32MB of flash */
 			reg = <0x30000000 0x02000000>;
 
-			/*
-			 * This "RedBoot" is the Storlink derivative.
-			 */
-			partition@0 {
-				label = "RedBoot";
-				reg = <0x00000000 0x00040000>;
-				read-only;
-			};
-			/*
-			 * This firmware image contains the kernel catenated
-			 * with the squashfs root filesystem. For some reason
-			 * this is called "upgrade" on the vendor system.
-			 */
-			partition@40000 {
-				label = "upgrade";
-				reg = <0x00040000 0x01f40000>;
-				read-only;
-			};
-			/* RGDB, Residental Gateway Database? */
-			partition@1f80000 {
-				label = "rgdb";
-				reg = <0x01f80000 0x00040000>;
-				read-only;
-			};
-			/*
-			 * This partition contains MAC addresses for WAN,
-			 * WLAN and LAN, and the country code (for wireless
-			 * I guess).
-			 */
-			partition@1fc0000 {
-				label = "nvram";
-				reg = <0x01fc0000 0x00020000>;
-				read-only;
-			};
-			partition@1fe0000 {
-				label = "LangPack";
-				reg = <0x01fe0000 0x00020000>;
-				read-only;
+			partitions {
+				compatible = "fixed-partitions";
+				#address-cells = <1>;
+				#size-cells = <1>;
+
+				/*
+				 * This "RedBoot" is the Storlink derivative.
+				 */
+				partition@0 {
+					label = "RedBoot";
+					reg = <0x00000000 0x00040000>;
+					read-only;
+				};
+				/*
+				 * This firmware image contains the kernel catenated
+				 * with the squashfs root filesystem. For some reason
+				 * this is called "upgrade" on the vendor system.
+				 */
+				partition@40000 {
+					label = "upgrade";
+					reg = <0x00040000 0x01f40000>;
+					read-only;
+				};
+				/* RGDB, Residental Gateway Database? */
+				partition@1f80000 {
+					label = "rgdb";
+					reg = <0x01f80000 0x00040000>;
+					read-only;
+				};
+				/*
+				 * This partition contains MAC addresses for WAN,
+				 * WLAN and LAN, and the country code (for wireless
+				 * I guess).
+				 */
+				partition@1fc0000 {
+					label = "nvram";
+					reg = <0x01fc0000 0x00020000>;
+					read-only;
+				};
+				partition@1fe0000 {
+					label = "LangPack";
+					reg = <0x01fe0000 0x00020000>;
+					read-only;
+				};
 			};
 		};
 
-- 
2.20.1

