From 06834226909bcb5bce5b5d0f7612258f8fe35201 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Thu, 2 Feb 2017 09:42:18 -0800
Subject: [PATCH 113/454] drm/vc4: Fix sending of page flip completion events
 in FKMS mode.

In the rewrite of vc4_crtc.c for fkms, I dropped the part of the
CRTC's atomic flush handler that moved the completion event from the
proposed atomic state change to the CRTC's current state.  That meant
that when full screen pageflipping happened (glxgears -fullscreen in
X, compton, por weston), the app would end up blocked firever waiting
to draw its next frame.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 drivers/gpu/drm/vc4/vc4_firmware_kms.c | 15 +++++++++++++++
 1 file changed, 15 insertions(+)

--- a/drivers/gpu/drm/vc4/vc4_firmware_kms.c
+++ b/drivers/gpu/drm/vc4/vc4_firmware_kms.c
@@ -336,6 +336,21 @@ static int vc4_crtc_atomic_check(struct
 static void vc4_crtc_atomic_flush(struct drm_crtc *crtc,
 				  struct drm_crtc_state *old_state)
 {
+	struct vc4_crtc *vc4_crtc = to_vc4_crtc(crtc);
+	struct drm_device *dev = crtc->dev;
+
+	if (crtc->state->event) {
+		unsigned long flags;
+
+		crtc->state->event->pipe = drm_crtc_index(crtc);
+
+		WARN_ON(drm_crtc_vblank_get(crtc) != 0);
+
+		spin_lock_irqsave(&dev->event_lock, flags);
+		vc4_crtc->event = crtc->state->event;
+		crtc->state->event = NULL;
+		spin_unlock_irqrestore(&dev->event_lock, flags);
+	}
 }
 
 static void vc4_crtc_handle_page_flip(struct vc4_crtc *vc4_crtc)
