From b2b8b06f18281c637da274b18e330bc52351637e Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Tue, 2 Jan 2018 10:58:27 +0000
Subject: [PATCH 292/454] net: mdiobus: add unlocked accessors

commit 34dc08e4be208539b7c4aa8154a610e1736705e8 upstream.

Add unlocked versions of the bus accessors, which allows access to the
bus with all the tracing. These accessors validate that the bus mutex
is held, which is a basic requirement for all mii bus accesses.

Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/phy/mdio_bus.c | 65 +++++++++++++++++++++++++++++++-------
 include/linux/mdio.h       |  3 ++
 2 files changed, 56 insertions(+), 12 deletions(-)

--- a/drivers/net/phy/mdio_bus.c
+++ b/drivers/net/phy/mdio_bus.c
@@ -493,6 +493,55 @@ struct phy_device *mdiobus_scan(struct m
 EXPORT_SYMBOL(mdiobus_scan);
 
 /**
+ * __mdiobus_read - Unlocked version of the mdiobus_read function
+ * @bus: the mii_bus struct
+ * @addr: the phy address
+ * @regnum: register number to read
+ *
+ * Read a MDIO bus register. Caller must hold the mdio bus lock.
+ *
+ * NOTE: MUST NOT be called from interrupt context.
+ */
+int __mdiobus_read(struct mii_bus *bus, int addr, u32 regnum)
+{
+	int retval;
+
+	WARN_ON_ONCE(!mutex_is_locked(&bus->mdio_lock));
+
+	retval = bus->read(bus, addr, regnum);
+
+	trace_mdio_access(bus, 1, addr, regnum, retval, retval);
+
+	return retval;
+}
+EXPORT_SYMBOL(__mdiobus_read);
+
+/**
+ * __mdiobus_write - Unlocked version of the mdiobus_write function
+ * @bus: the mii_bus struct
+ * @addr: the phy address
+ * @regnum: register number to write
+ * @val: value to write to @regnum
+ *
+ * Write a MDIO bus register. Caller must hold the mdio bus lock.
+ *
+ * NOTE: MUST NOT be called from interrupt context.
+ */
+int __mdiobus_write(struct mii_bus *bus, int addr, u32 regnum, u16 val)
+{
+	int err;
+
+	WARN_ON_ONCE(!mutex_is_locked(&bus->mdio_lock));
+
+	err = bus->write(bus, addr, regnum, val);
+
+	trace_mdio_access(bus, 0, addr, regnum, val, err);
+
+	return err;
+}
+EXPORT_SYMBOL(__mdiobus_write);
+
+/**
  * mdiobus_read_nested - Nested version of the mdiobus_read function
  * @bus: the mii_bus struct
  * @addr: the phy address
@@ -512,11 +561,9 @@ int mdiobus_read_nested(struct mii_bus *
 	BUG_ON(in_interrupt());
 
 	mutex_lock_nested(&bus->mdio_lock, MDIO_MUTEX_NESTED);
-	retval = bus->read(bus, addr, regnum);
+	retval = __mdiobus_read(bus, addr, regnum);
 	mutex_unlock(&bus->mdio_lock);
 
-	trace_mdio_access(bus, 1, addr, regnum, retval, retval);
-
 	return retval;
 }
 EXPORT_SYMBOL(mdiobus_read_nested);
@@ -538,11 +585,9 @@ int mdiobus_read(struct mii_bus *bus, in
 	BUG_ON(in_interrupt());
 
 	mutex_lock(&bus->mdio_lock);
-	retval = bus->read(bus, addr, regnum);
+	retval = __mdiobus_read(bus, addr, regnum);
 	mutex_unlock(&bus->mdio_lock);
 
-	trace_mdio_access(bus, 1, addr, regnum, retval, retval);
-
 	return retval;
 }
 EXPORT_SYMBOL(mdiobus_read);
@@ -568,11 +613,9 @@ int mdiobus_write_nested(struct mii_bus
 	BUG_ON(in_interrupt());
 
 	mutex_lock_nested(&bus->mdio_lock, MDIO_MUTEX_NESTED);
-	err = bus->write(bus, addr, regnum, val);
+	err = __mdiobus_write(bus, addr, regnum, val);
 	mutex_unlock(&bus->mdio_lock);
 
-	trace_mdio_access(bus, 0, addr, regnum, val, err);
-
 	return err;
 }
 EXPORT_SYMBOL(mdiobus_write_nested);
@@ -595,11 +638,9 @@ int mdiobus_write(struct mii_bus *bus, i
 	BUG_ON(in_interrupt());
 
 	mutex_lock(&bus->mdio_lock);
-	err = bus->write(bus, addr, regnum, val);
+	err = __mdiobus_write(bus, addr, regnum, val);
 	mutex_unlock(&bus->mdio_lock);
 
-	trace_mdio_access(bus, 0, addr, regnum, val, err);
-
 	return err;
 }
 EXPORT_SYMBOL(mdiobus_write);
--- a/include/linux/mdio.h
+++ b/include/linux/mdio.h
@@ -257,6 +257,9 @@ static inline u16 ethtool_adv_to_mmd_eee
 	return reg;
 }
 
+int __mdiobus_read(struct mii_bus *bus, int addr, u32 regnum);
+int __mdiobus_write(struct mii_bus *bus, int addr, u32 regnum, u16 val);
+
 int mdiobus_read(struct mii_bus *bus, int addr, u32 regnum);
 int mdiobus_read_nested(struct mii_bus *bus, int addr, u32 regnum);
 int mdiobus_write(struct mii_bus *bus, int addr, u32 regnum, u16 val);
