From 0aa052ce1c3340850a7e5980b6d24b3ea5779591 Mon Sep 17 00:00:00 2001
From: Dan Haab <dhaab@luxul.com>
Date: Mon, 9 Oct 2017 09:46:59 -0600
Subject: [PATCH] ARM: dts: BCM53573: Add DT for Luxul XAP-810
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This is BCM53573 WiSoC based access point with an extra BCM43217 chipset
used for 2.4 GHz.

Signed-off-by: Dan Haab <dhaab@luxul.com>
Acked-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/Makefile                   |  1 +
 arch/arm/boot/dts/bcm47189-luxul-xap-810.dts | 87 ++++++++++++++++++++++++++++
 2 files changed, 88 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm47189-luxul-xap-810.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -111,6 +111,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm953012hr.dtb \
 	bcm953012k.dtb
 dtb-$(CONFIG_ARCH_BCM_53573) += \
+	bcm47189-luxul-xap-810.dtb \
 	bcm47189-tenda-ac9.dtb \
 	bcm947189acdbmr.dtb
 dtb-$(CONFIG_ARCH_BCM_63XX) += \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47189-luxul-xap-810.dts
@@ -0,0 +1,87 @@
+/*
+ * Copyright 2017 Luxul Inc.
+ *
+ * Licensed under the ISC license.
+ */
+
+/dts-v1/;
+
+#include "bcm53573.dtsi"
+
+/ {
+	compatible = "luxul,xap-810-v1", "brcm,bcm47189", "brcm,bcm53573";
+	model = "Luxul XAP-810 V1";
+
+	chosen {
+		bootargs = "earlycon";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		5ghz {
+			label = "bcm53xx:blue:5ghz";
+			gpios = <&chipcommon 11 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+
+		system {
+			label = "bcm53xx:green:system";
+			gpios = <&chipcommon 15 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "timer";
+		};
+	};
+
+	pcie0_leds {
+		compatible = "gpio-leds";
+
+		2ghz {
+			label = "bcm53xx:blue:2ghz";
+			gpios = <&pcie0_chipcommon 3 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-off";
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 7 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&pcie0 {
+	ranges = <0x00000000 0 0 0 0 0x00100000>;
+	#address-cells = <3>;
+	#size-cells = <2>;
+
+	bridge@0,0,0 {
+		reg = <0x0000 0 0 0 0>;
+		ranges = <0x00000000 0 0 0 0 0 0 0x00100000>;
+		#address-cells = <3>;
+		#size-cells = <2>;
+
+		wifi@0,1,0 {
+			reg = <0x0000 0 0 0 0>;
+			ranges = <0x00000000 0 0 0 0x00100000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			pcie0_chipcommon: chipcommon@0 {
+				reg = <0 0x1000>;
+
+				gpio-controller;
+				#gpio-cells = <2>;
+			};
+		};
+	};
+};
