From patchwork Mon May 21 20:57:38 2018
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
Subject: [v5,3/4] ARM: dts: qcom: add gpio-ranges property
X-Patchwork-Submitter: Christian Lamparter <chunkeey@gmail.com>
X-Patchwork-Id: 917856
Message-Id: <0ae3376606a89bcdf3fe753a5c967f7103699e09.1526935804.git.chunkeey@gmail.com>
To: linux-gpio@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
 linux-arm-msm@vger.kernel.org, devicetree@vger.kernel.org
Cc: Bjorn Andersson <bjorn.andersson@linaro.org>,
 Linus Walleij <linus.walleij@linaro.org>,
 Stephen Boyd <sboyd@kernel.org>, David Brown <david.brown@linaro.org>,
 Rob Herring <robh+dt@kernel.org>, Mark Rutland <mark.rutland@arm.com>,
 Andy Gross <andy.gross@linaro.org>,
 Sven Eckelmann <sven.eckelmann@openmesh.com>
Date: Mon, 21 May 2018 22:57:38 +0200
From: Christian Lamparter <chunkeey@gmail.com>
List-Id: <linux-gpio.vger.kernel.org>

This patch adds the gpio-ranges property to almost all of
the Qualcomm ARM platforms that utilize the pinctrl-msm
framework.

The gpio-ranges property is part of the gpiolib subsystem.
As a result, the binding text is available in section
"2.1 gpio- and pin-controller interaction" of
Documentation/devicetree/bindings/gpio/gpio.txt

For more information please see the patch titled:
"pinctrl: msm: fix gpio-hog related boot issues" from
this series.

Reported-by: Sven Eckelmann <sven.eckelmann@openmesh.com>
Tested-by: Sven Eckelmann <sven.eckelmann@openmesh.com> [ipq4019]
Reviewed-by: Bjorn Andersson <bjorn.andersson@linaro.org>
Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
Reviewed-by: Linus Walleij <linus.walleij@linaro.org>
---
To help with git bisect, the DT update patch has been intentionally
placed after the "pinctrl: msm: fix gpio-hog related boot issues".
Otherwise - if the order was reveresed - and bisect decides to split
between these two patches, the gpiochip_add_pin_ranges() function
will be executed twice with the same parameters for the same pinctrl.
---
 arch/arm/boot/dts/qcom-apq8064.dtsi   | 1 +
 arch/arm/boot/dts/qcom-apq8084.dtsi   | 1 +
 arch/arm/boot/dts/qcom-ipq4019.dtsi   | 1 +
 arch/arm/boot/dts/qcom-ipq8064.dtsi   | 1 +
 arch/arm/boot/dts/qcom-mdm9615.dtsi   | 1 +
 arch/arm/boot/dts/qcom-msm8660.dtsi   | 1 +
 arch/arm/boot/dts/qcom-msm8960.dtsi   | 1 +
 arch/arm/boot/dts/qcom-msm8974.dtsi   | 1 +
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 3 ++-
 arch/arm64/boot/dts/qcom/msm8916.dtsi | 1 +
 arch/arm64/boot/dts/qcom/msm8992.dtsi | 1 +
 arch/arm64/boot/dts/qcom/msm8994.dtsi | 1 +
 arch/arm64/boot/dts/qcom/msm8996.dtsi | 1 +
 13 files changed, 14 insertions(+), 1 deletion(-)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -202,6 +202,7 @@
 			compatible = "qcom,ipq4019-pinctrl";
 			reg = <0x01000000 0x300000>;
 			gpio-controller;
+			gpio-ranges = <&tlmm 0 0 100>;
 			#gpio-cells = <2>;
 			interrupt-controller;
 			#interrupt-cells = <2>;
