#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "zyxel,p-2812hnu", "lantiq,xway", "lantiq,vr9";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &dsl_green;
		led-internet = &internet_green;
		led-wifi = &wireless_green;
	};

	memory@0 {
		reg = <0x0 0x8000000>;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 39 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		rfkill {
			label = "rfkill";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		internet_red {
			label = "p2812hnufx:red:internet";
			gpios = <&stp 16 GPIO_ACTIVE_LOW>;
		};
		internet_green: internet_green {
			label = "p2812hnufx:green:internet";
			gpios = <&stp 17 GPIO_ACTIVE_LOW>;
		};
		dsl_green: dsl_green {
			label = "p2812hnufx:green:dsl";
			gpios = <&stp 18 GPIO_ACTIVE_LOW>;
		};
		dsl_orange {
			label = "p2812hnufx:orange:dsl";
			gpios = <&stp 19 GPIO_ACTIVE_LOW>;
		};
		wireless_orange {
			label = "p2812hnufx:orange:wlan";
			gpios = <&stp 20 GPIO_ACTIVE_LOW>;
		};
		wireless_green: wireless_green {
			label = "p2812hnufx:green:wlan";
			gpios = <&stp 21 GPIO_ACTIVE_LOW>;
		};
		power_red: power {
			label = "p2812hnufx:red:power";
			gpios = <&stp 22 GPIO_ACTIVE_LOW>;
		};
		power_green: power2 {
			label = "p2812hnufx:green:power";
			gpios = <&stp 23 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		phone1 {
			label = "p2812hnufx:green:phone";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
		phone1warn {
			label = "p2812hnufx:orange:phone";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};
		phone2warn {
			label = "p2812hnufx:orange:phone2";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};
		phone2 {
			label = "p2812hnufx:green:phone2";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 33 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&eth0 {
	lan: interface@0 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;
		mac-address = [ 00 11 22 33 44 55 ];
		lantiq,switch;

		ethernet@0 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <0>;
			phy-mode = "rgmii";
			phy-handle = <&phy0>;
		};
		ethernet@1 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <1>;
			phy-mode = "rgmii";
			phy-handle = <&phy1>;
		};
		ethernet@2 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <2>;
			phy-mode = "gmii";
			phy-handle = <&phy11>;
		};
		ethernet@4 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <4>;
			phy-mode = "gmii";
			phy-handle = <&phy13>;
		};
		ethernet@5 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <5>;
			phy-mode = "rgmii";
			phy-handle = <&phy5>;
		};
	};

	mdio@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";
		reg = <0>;

		phy0: ethernet-phy@0 {
			reg = <0x0>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy1: ethernet-phy@1 {
			reg = <0x1>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy5: ethernet-phy@5 {
			reg = <0x5>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy11: ethernet-phy@11 {
			reg = <0x11>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy13: ethernet-phy@13 {
			reg = <0x13>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
	};
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		exin3 {
			lantiq,groups = "exin3";
			lantiq,function = "exin";
		};
		mdio {
			lantiq,groups = "mdio";
			lantiq,function = "mdio";
		};
		gphy-leds {
			lantiq,groups = "gphy0 led1", "gphy1 led1",
					"gphy0 led2", "gphy1 led2";
			lantiq,function = "gphy";
			lantiq,pull = <2>;
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
		stp {
			lantiq,groups = "stp";
			lantiq,function = "stp";
			lantiq,pull = <2>;
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
		pci-in {
			lantiq,groups = "req1";
			lantiq,function = "pci";
			lantiq,output = <0>;
			lantiq,open-drain = <1>;
			lantiq,pull = <2>;
		};
		pci-out {
			lantiq,groups = "gnt1";
			lantiq,function = "pci";
			lantiq,output = <1>;
			lantiq,open-drain = <0>;
			lantiq,pull = <0>;
		};
		pci_rst {
			lantiq,pins = "io21";
			lantiq,output = <1>;
			lantiq,open-drain = <0>;
			lantiq,pull = <2>;
		};
		pcie-rst {
			lantiq,pins = "io38";
			lantiq,pull = <0>;
			lantiq,output = <1>;
		};
		ifxhcd-rst {
			lantiq,pins = "io33";
			lantiq,pull = <0>;
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
		nand_out {
			lantiq,groups = "nand cle", "nand ale";
			lantiq,function = "ebu";
			lantiq,output = <1>;
			lantiq,open-drain = <0>;
			lantiq,pull = <0>;
		};
		nand_cs1 {
			lantiq,groups = "nand cs1";
			lantiq,function = "ebu";
			lantiq,open-drain = <0>;
			lantiq,pull = <0>;
		};
	};
};

&pci0 {
	status = "okay";
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;
};

&stp {
	status = "okay";

	lantiq,shadow = <0xffffff>;
	lantiq,groups = <0x7>;
	lantiq,dsl = <0x0>;
	lantiq,phy1 = <0x0>;
	lantiq,phy2 = <0x0>;
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb0 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&usb1 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};
