--- a/arch/arm/boot/dts/mt7623n-bananapi-bpi-r2.dts
+++ b/arch/arm/boot/dts/mt7623n-bananapi-bpi-r2.dts
@@ -21,6 +21,10 @@
 		stdout-path = "serial2:115200n8";
 	};
 
+	memory {
+		reg = <0 0x80000000 0 0x20000000>;
+	};
+
 	cpus {
 		cpu@0 {
 			proc-supply = <&mt6323_vproc_reg>;
@@ -103,6 +107,10 @@
 		device_type = "memory";
 		reg = <0 0x80000000 0 0x40000000>;
 	};
+
+	mt7530: switch@0 {
+		compatible = "mediatek,mt7530";
+	};
 };
 
 &cir {
@@ -130,11 +138,24 @@
 		};
 	};
 
+	gmac1: mac@1 {
+		compatible = "mediatek,eth-mac";
+		reg = <1>;
+		phy-mode = "rgmii";
+
+		fixed-link {
+			speed = <1000>;
+			full-duplex;
+			pause;
+		};
+	};
+
 	mdio: mdio-bus {
 		#address-cells = <1>;
 		#size-cells = <0>;
-
-		switch@0 {
+	};
+};
+		&mt7530 {
 			compatible = "mediatek,mt7530";
 			#address-cells = <1>;
 			#size-cells = <0>;
@@ -144,6 +165,8 @@
 			core-supply = <&mt6323_vpa_reg>;
 			io-supply = <&mt6323_vemc3v3_reg>;
 
+			dsa,mii-bus = <&mdio>;
+
 			ports {
 				#address-cells = <1>;
 				#size-cells = <0>;
@@ -152,29 +175,46 @@
 				port@0 {
 					reg = <0>;
 					label = "wan";
+					cpu = <&cpu_port1>;
 				};
 
 				port@1 {
 					reg = <1>;
 					label = "lan0";
+					cpu = <&cpu_port0>;
 				};
 
 				port@2 {
 					reg = <2>;
 					label = "lan1";
+					cpu = <&cpu_port0>;
 				};
 
 				port@3 {
 					reg = <3>;
 					label = "lan2";
+					cpu = <&cpu_port0>;
 				};
 
 				port@4 {
 					reg = <4>;
 					label = "lan3";
+					cpu = <&cpu_port0>;
 				};
 
-				port@6 {
+				cpu_port1: port@5 {
+					reg = <5>;
+					label = "cpu";
+					ethernet = <&gmac1>;
+					phy-mode = "rgmii";
+
+					fixed-link {
+						speed = <1000>;
+						full-duplex;
+					};
+				};
+
+				cpu_port0: port@6 {
 					reg = <6>;
 					label = "cpu";
 					ethernet = <&gmac0>;
@@ -188,8 +228,6 @@
 				};
 			};
 		};
-	};
-};
 
 &i2c0 {
 	pinctrl-names = "default";
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -1061,6 +1061,7 @@ dtb-$(CONFIG_ARCH_MEDIATEK) += \
 	mt6580-evbp1.dtb \
 	mt6589-aquaris5.dtb \
 	mt6592-evb.dtb \
+	mt7623a-rfb-emmc.dtb \
 	mt7623n-rfb-nand.dtb \
 	mt7623n-bananapi-bpi-r2.dtb \
 	mt8127-moose.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/mt7623a-rfb-emmc.dts
@@ -0,0 +1,449 @@
+/*
+ * Copyright 2017 Sean Wang <sean.wang@mediatek.com>
+ *
+ * SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+ */
+
+/dts-v1/;
+#include <dt-bindings/input/input.h>
+#include "mt7623.dtsi"
+#include "mt6323.dtsi"
+
+/ {
+	model = "MediaTek MT7623N NAND reference board";
+	compatible = "mediatek,mt7623a-rfb-emmc", "mediatek,mt7623";
+
+	aliases {
+		serial2 = &uart2;
+	};
+
+	chosen {
+		bootargs = "earlyprintk block2mtd.block2mtd=/dev/mmcblk0,65536,eMMC,5 mtdparts=eMMC:256k(mbr)ro,512k(uboot)ro,256k(config)ro,256k(factory)ro,32M(kernel),32M(recovery),1024M(rootfs),2048M(usrdata),-(bmtpool) rootfstype=squashfs,jffs2";
+
+		stdout-path = "serial2:115200n8";
+	};
+
+	memory {
+		reg = <0 0x80000000 0 0x20000000>;
+	};
+
+	cpus {
+		cpu@0 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+
+		cpu@1 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+
+		cpu@2 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+
+		cpu@3 {
+			proc-supply = <&mt6323_vproc_reg>;
+		};
+	};
+
+	memory@80000000 {
+		reg = <0 0x80000000 0 0x40000000>;
+	};
+
+	mt7530: switch@0 {
+		compatible = "mediatek,mt7530";
+		#address-cells = <1>;
+		#size-cells = <0>;
+	};
+};
+
+&crypto {
+	status = "okay";
+};
+
+&eth {
+	status = "okay";
+
+	gmac0: mac@0 {
+		compatible = "mediatek,eth-mac";
+		reg = <0>;
+		phy-mode = "trgmii";
+
+		fixed-link {
+			speed = <1000>;
+			full-duplex;
+			pause;
+		};
+	};
+
+	gmac1: mac@1 {
+		compatible = "mediatek,eth-mac";
+		reg = <1>;
+		phy-mode = "rgmiii-rxid";
+		phy-handle = <&phy5>;
+	};
+
+	mdio: mdio-bus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		phy5: ethernet-phy@5 {
+			reg = <5>;
+			phy-mode = "rgmii-rxid";
+		};
+	};
+};
+
+&mt7530 {
+	compatible = "mediatek,mt7530";
+	#address-cells = <1>;
+	#size-cells = <0>;
+	reg = <0>;
+	pinctrl-names = "default";
+	mediatek,mcm;
+	resets = <&ethsys 2>;
+	reset-names = "mcm";
+	core-supply = <&mt6323_vpa_reg>;
+	io-supply = <&mt6323_vemc3v3_reg>;
+
+	dsa,mii-bus = <&mdio>;
+
+	ports {
+		#address-cells = <1>;
+		#size-cells = <0>;
+		reg = <0>;
+
+		port@0 {
+			reg = <0>;
+			label = "lan0";
+			cpu = <&cpu_port0>;
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan1";
+			cpu = <&cpu_port0>;
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan2";
+			cpu = <&cpu_port0>;
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan3";
+			cpu = <&cpu_port0>;
+		};
+
+		cpu_port0: port@6 {
+			reg = <6>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+			phy-mode = "trgmii";
+
+			fixed-link {
+				speed = <1000>;
+				full-duplex;
+			};
+		};
+	};
+};
+
+&i2c0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c0_pins_a>;
+	status = "okay";
+};
+
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins_a>;
+	status = "okay";
+};
+
+&mmc0 {
+	pinctrl-names = "default", "state_uhs";
+	pinctrl-0 = <&mmc0_pins_default>;
+	pinctrl-1 = <&mmc0_pins_uhs>;
+	status = "okay";
+	bus-width = <8>;
+	max-frequency = <50000000>;
+	cap-mmc-highspeed;
+	vmmc-supply = <&mt6323_vemc3v3_reg>;
+	vqmmc-supply = <&mt6323_vio18_reg>;
+	non-removable;
+};
+
+&mmc1 {
+	pinctrl-names = "default", "state_uhs";
+	pinctrl-0 = <&mmc1_pins_default>;
+	pinctrl-1 = <&mmc1_pins_uhs>;
+	status = "okay";
+	bus-width = <4>;
+	max-frequency = <50000000>;
+	cap-sd-highspeed;
+	cd-gpios = <&pio 261 0>;
+	vmmc-supply = <&mt6323_vmch_reg>;
+	vqmmc-supply = <&mt6323_vio18_reg>;
+};
+
+&pio {
+	cir_pins_a:cir@0 {
+		pins_cir {
+			pinmux = <MT7623_PIN_46_IR_FUNC_IR>;
+			bias-disable;
+		};
+	};
+
+	i2c0_pins_a: i2c@0 {
+		pins_i2c0 {
+			pinmux = <MT7623_PIN_75_SDA0_FUNC_SDA0>,
+				 <MT7623_PIN_76_SCL0_FUNC_SCL0>;
+			bias-disable;
+		};
+	};
+
+	i2c1_pins_a: i2c@1 {
+		pin_i2c1 {
+			pinmux = <MT7623_PIN_57_SDA1_FUNC_SDA1>,
+				 <MT7623_PIN_58_SCL1_FUNC_SCL1>;
+			bias-disable;
+		};
+	};
+
+	i2s0_pins_a: i2s@0 {
+		pin_i2s0 {
+			pinmux = <MT7623_PIN_49_I2S0_DATA_FUNC_I2S0_DATA>,
+				 <MT7623_PIN_72_I2S0_DATA_IN_FUNC_I2S0_DATA_IN>,
+				 <MT7623_PIN_73_I2S0_LRCK_FUNC_I2S0_LRCK>,
+				 <MT7623_PIN_74_I2S0_BCK_FUNC_I2S0_BCK>,
+				 <MT7623_PIN_126_I2S0_MCLK_FUNC_I2S0_MCLK>;
+			drive-strength = <MTK_DRIVE_12mA>;
+			bias-pull-down;
+		};
+	};
+
+	i2s1_pins_a: i2s@1 {
+		pin_i2s1 {
+			pinmux = <MT7623_PIN_33_I2S1_DATA_FUNC_I2S1_DATA>,
+				 <MT7623_PIN_34_I2S1_DATA_IN_FUNC_I2S1_DATA_IN>,
+				 <MT7623_PIN_35_I2S1_BCK_FUNC_I2S1_BCK>,
+				 <MT7623_PIN_36_I2S1_LRCK_FUNC_I2S1_LRCK>,
+				 <MT7623_PIN_37_I2S1_MCLK_FUNC_I2S1_MCLK>;
+			drive-strength = <MTK_DRIVE_12mA>;
+			bias-pull-down;
+		};
+	};
+
+	mmc0_pins_default: mmc0default {
+		pins_cmd_dat {
+			pinmux = <MT7623_PIN_111_MSDC0_DAT7_FUNC_MSDC0_DAT7>,
+				 <MT7623_PIN_112_MSDC0_DAT6_FUNC_MSDC0_DAT6>,
+				 <MT7623_PIN_113_MSDC0_DAT5_FUNC_MSDC0_DAT5>,
+				 <MT7623_PIN_114_MSDC0_DAT4_FUNC_MSDC0_DAT4>,
+				 <MT7623_PIN_118_MSDC0_DAT3_FUNC_MSDC0_DAT3>,
+				 <MT7623_PIN_119_MSDC0_DAT2_FUNC_MSDC0_DAT2>,
+				 <MT7623_PIN_120_MSDC0_DAT1_FUNC_MSDC0_DAT1>,
+				 <MT7623_PIN_121_MSDC0_DAT0_FUNC_MSDC0_DAT0>,
+				 <MT7623_PIN_116_MSDC0_CMD_FUNC_MSDC0_CMD>;
+			input-enable;
+			bias-pull-up;
+		};
+
+		pins_clk {
+			pinmux = <MT7623_PIN_117_MSDC0_CLK_FUNC_MSDC0_CLK>;
+			bias-pull-down;
+		};
+
+		pins_rst {
+			pinmux = <MT7623_PIN_115_MSDC0_RSTB_FUNC_MSDC0_RSTB>;
+			bias-pull-up;
+		};
+	};
+
+	mmc0_pins_uhs: mmc0 {
+		pins_cmd_dat {
+			pinmux = <MT7623_PIN_111_MSDC0_DAT7_FUNC_MSDC0_DAT7>,
+				 <MT7623_PIN_112_MSDC0_DAT6_FUNC_MSDC0_DAT6>,
+				 <MT7623_PIN_113_MSDC0_DAT5_FUNC_MSDC0_DAT5>,
+				 <MT7623_PIN_114_MSDC0_DAT4_FUNC_MSDC0_DAT4>,
+				 <MT7623_PIN_118_MSDC0_DAT3_FUNC_MSDC0_DAT3>,
+				 <MT7623_PIN_119_MSDC0_DAT2_FUNC_MSDC0_DAT2>,
+				 <MT7623_PIN_120_MSDC0_DAT1_FUNC_MSDC0_DAT1>,
+				 <MT7623_PIN_121_MSDC0_DAT0_FUNC_MSDC0_DAT0>,
+				 <MT7623_PIN_116_MSDC0_CMD_FUNC_MSDC0_CMD>;
+			input-enable;
+			drive-strength = <MTK_DRIVE_2mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_01>;
+		};
+
+		pins_clk {
+			pinmux = <MT7623_PIN_117_MSDC0_CLK_FUNC_MSDC0_CLK>;
+			drive-strength = <MTK_DRIVE_2mA>;
+			bias-pull-down = <MTK_PUPD_SET_R1R0_01>;
+		};
+
+		pins_rst {
+			pinmux = <MT7623_PIN_115_MSDC0_RSTB_FUNC_MSDC0_RSTB>;
+			bias-pull-up;
+		};
+	};
+
+	mmc1_pins_default: mmc1default {
+		pins_cmd_dat {
+			pinmux = <MT7623_PIN_107_MSDC1_DAT0_FUNC_MSDC1_DAT0>,
+				 <MT7623_PIN_108_MSDC1_DAT1_FUNC_MSDC1_DAT1>,
+				 <MT7623_PIN_109_MSDC1_DAT2_FUNC_MSDC1_DAT2>,
+				 <MT7623_PIN_110_MSDC1_DAT3_FUNC_MSDC1_DAT3>,
+				 <MT7623_PIN_105_MSDC1_CMD_FUNC_MSDC1_CMD>;
+			input-enable;
+			drive-strength = <MTK_DRIVE_4mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_10>;
+		};
+
+		pins_clk {
+			pinmux = <MT7623_PIN_106_MSDC1_CLK_FUNC_MSDC1_CLK>;
+			bias-pull-down;
+			drive-strength = <MTK_DRIVE_4mA>;
+		};
+
+		pins_wp {
+			pinmux = <MT7623_PIN_29_EINT7_FUNC_MSDC1_WP>;
+			input-enable;
+			bias-pull-up;
+		};
+
+		pins_insert {
+			pinmux = <MT7623_PIN_261_MSDC1_INS_FUNC_GPIO261>;
+			bias-pull-up;
+		};
+	};
+
+	mmc1_pins_uhs: mmc1 {
+		pins_cmd_dat {
+			pinmux = <MT7623_PIN_107_MSDC1_DAT0_FUNC_MSDC1_DAT0>,
+				 <MT7623_PIN_108_MSDC1_DAT1_FUNC_MSDC1_DAT1>,
+				 <MT7623_PIN_109_MSDC1_DAT2_FUNC_MSDC1_DAT2>,
+				 <MT7623_PIN_110_MSDC1_DAT3_FUNC_MSDC1_DAT3>,
+				 <MT7623_PIN_105_MSDC1_CMD_FUNC_MSDC1_CMD>;
+			input-enable;
+			drive-strength = <MTK_DRIVE_4mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_10>;
+		};
+
+		pins_clk {
+			pinmux = <MT7623_PIN_106_MSDC1_CLK_FUNC_MSDC1_CLK>;
+			drive-strength = <MTK_DRIVE_4mA>;
+			bias-pull-down = <MTK_PUPD_SET_R1R0_10>;
+		};
+	};
+
+	pwm_pins_a: pwm@0 {
+		pins_pwm {
+			pinmux = <MT7623_PIN_203_PWM0_FUNC_PWM0>,
+				 <MT7623_PIN_204_PWM1_FUNC_PWM1>,
+				 <MT7623_PIN_205_PWM2_FUNC_PWM2>,
+				 <MT7623_PIN_206_PWM3_FUNC_PWM3>,
+				 <MT7623_PIN_207_PWM4_FUNC_PWM4>;
+		};
+	};
+
+	spi0_pins_a: spi@0 {
+		pins_spi {
+			pinmux = <MT7623_PIN_53_SPI0_CSN_FUNC_SPI0_CS>,
+				<MT7623_PIN_54_SPI0_CK_FUNC_SPI0_CK>,
+				<MT7623_PIN_55_SPI0_MI_FUNC_SPI0_MI>,
+				<MT7623_PIN_56_SPI0_MO_FUNC_SPI0_MO>;
+			bias-disable;
+		};
+	};
+
+	uart0_pins_a: uart@0 {
+		pins_dat {
+			pinmux = <MT7623_PIN_79_URXD0_FUNC_URXD0>,
+				 <MT7623_PIN_80_UTXD0_FUNC_UTXD0>;
+		};
+	};
+
+	uart1_pins_a: uart@1 {
+		pins_dat {
+			pinmux = <MT7623_PIN_81_URXD1_FUNC_URXD1>,
+				 <MT7623_PIN_82_UTXD1_FUNC_UTXD1>;
+		};
+	};
+};
+
+&pwm {
+	pinctrl-names = "default";
+	pinctrl-0 = <&pwm_pins_a>;
+	status = "okay";
+};
+
+&pwrap {
+	mt6323 {
+		mt6323led: led {
+			compatible = "mediatek,mt6323-led";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			led@0 {
+				reg = <0>;
+				label = "bpi-r2:isink:green";
+				default-state = "off";
+			};
+
+			led@1 {
+				reg = <1>;
+				label = "bpi-r2:isink:red";
+				default-state = "off";
+			};
+
+			led@2 {
+				reg = <2>;
+				label = "bpi-r2:isink:blue";
+				default-state = "off";
+			};
+		};
+	};
+};
+
+&spi0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi0_pins_a>;
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins_a>;
+	status = "disabled";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins_a>;
+	status = "disabled";
+};
+
+&uart2 {
+	status = "okay";
+};
+
+&usb1 {
+	vusb33-supply = <&mt6323_vusb_reg>;
+	status = "okay";
+};
+
+&usb2 {
+	vusb33-supply = <&mt6323_vusb_reg>;
+	status = "okay";
+};
+
+&u3phy1 {
+	status = "okay";
+};
+
+&u3phy2 {
+	status = "okay";
+};
+
--- a/arch/arm/boot/dts/mt7623.dtsi
+++ b/arch/arm/boot/dts/mt7623.dtsi
@@ -326,6 +326,7 @@
 			     "syscon";
 		reg = <0 0x10209000 0 0x1000>;
 		#clock-cells = <1>;
+		#reset-cells = <1>;
 	};
 
 	rng: rng@1020f000 {
