From ca576b3fd93dff35bdf39f5fd44edf938e545ac9 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Thu, 5 Jul 2018 16:43:56 +0100
Subject: [PATCH 341/454] BCM283x DT: Add CSI nodes to the device tree.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2708-rpi.dtsi            |  8 ++++++
 arch/arm/boot/dts/bcm2835-rpi-a-plus.dts      |  1 +
 arch/arm/boot/dts/bcm2835-rpi-a.dts           |  1 +
 arch/arm/boot/dts/bcm2835-rpi-b-plus.dts      |  1 +
 arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts      |  1 +
 arch/arm/boot/dts/bcm2835-rpi-b.dts           |  1 +
 arch/arm/boot/dts/bcm2835-rpi-zero.dts        |  1 +
 arch/arm/boot/dts/bcm2835-rpi.dtsi            |  8 ++++++
 arch/arm/boot/dts/bcm2836-rpi-2-b.dts         |  1 +
 arch/arm/boot/dts/bcm2837-rpi-3-b.dts         |  1 +
 arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi |  7 +++++
 arch/arm/boot/dts/bcm283x.dtsi                | 28 +++++++++++++++++++
 .../dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi  |  1 +
 13 files changed, 60 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi
 create mode 120000 arch/arm64/boot/dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi

--- a/arch/arm/boot/dts/bcm2708-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2708-rpi.dtsi
@@ -160,3 +160,11 @@ sdhost_pins: &sdhost_gpio48 {
 &vec {
 	status = "disabled";
 };
+
+&csi0 {
+	power-domains = <&power RPI_POWER_DOMAIN_UNICAM0>;
+};
+
+&csi1 {
+	power-domains = <&power RPI_POWER_DOMAIN_UNICAM1>;
+};
--- a/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-a-plus.dts
@@ -3,6 +3,7 @@
 #include "bcm2835.dtsi"
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-usb-host.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,model-a-plus", "brcm,bcm2835";
--- a/arch/arm/boot/dts/bcm2835-rpi-a.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-a.dts
@@ -3,6 +3,7 @@
 #include "bcm2835.dtsi"
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-usb-host.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,model-a", "brcm,bcm2835";
--- a/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b-plus.dts
@@ -4,6 +4,7 @@
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-smsc9514.dtsi"
 #include "bcm283x-rpi-usb-host.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,model-b-plus", "brcm,bcm2835";
--- a/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b-rev2.dts
@@ -4,6 +4,7 @@
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-smsc9512.dtsi"
 #include "bcm283x-rpi-usb-host.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,model-b-rev2", "brcm,bcm2835";
--- a/arch/arm/boot/dts/bcm2835-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-b.dts
@@ -4,6 +4,7 @@
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-smsc9512.dtsi"
 #include "bcm283x-rpi-usb-host.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,model-b", "brcm,bcm2835";
--- a/arch/arm/boot/dts/bcm2835-rpi-zero.dts
+++ b/arch/arm/boot/dts/bcm2835-rpi-zero.dts
@@ -13,6 +13,7 @@
 #include "bcm2835.dtsi"
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-usb-otg.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,model-zero", "brcm,bcm2835";
--- a/arch/arm/boot/dts/bcm2835-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2835-rpi.dtsi
@@ -106,3 +106,11 @@
 &dsi1 {
 	power-domains = <&power RPI_POWER_DOMAIN_DSI1>;
 };
+
+&csi0 {
+	power-domains = <&power RPI_POWER_DOMAIN_UNICAM0>;
+};
+
+&csi1 {
+	power-domains = <&power RPI_POWER_DOMAIN_UNICAM1>;
+};
--- a/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
+++ b/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
@@ -4,6 +4,7 @@
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-smsc9514.dtsi"
 #include "bcm283x-rpi-usb-host.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,2-model-b", "brcm,bcm2836";
--- a/arch/arm/boot/dts/bcm2837-rpi-3-b.dts
+++ b/arch/arm/boot/dts/bcm2837-rpi-3-b.dts
@@ -4,6 +4,7 @@
 #include "bcm2835-rpi.dtsi"
 #include "bcm283x-rpi-smsc9514.dtsi"
 #include "bcm283x-rpi-usb-host.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,3-model-b", "brcm,bcm2837";
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-csi1-2lane.dtsi
@@ -0,0 +1,7 @@
+&csi1 {
+	port {
+		endpoint {
+			data-lanes = <1 2>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm283x.dtsi
+++ b/arch/arm/boot/dts/bcm283x.dtsi
@@ -545,6 +545,34 @@
 			status = "disabled";
 		};
 
+		csi0: csi0@7e800000 {
+			compatible = "brcm,bcm2835-unicam";
+			reg = <0x7e800000 0x800>,
+			      <0x7e802000 0x4>;
+			interrupts = <2 6>;
+			clocks = <&clocks BCM2835_CLOCK_CAM0>;
+			clock-names = "lp";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			#clock-cells = <1>;
+
+			status = "disabled";
+		};
+
+		csi1: csi1@7e801000 {
+			compatible = "brcm,bcm2835-unicam";
+			reg = <0x7e801000 0x800>,
+			      <0x7e802004 0x4>;
+			interrupts = <2 7>;
+			clocks = <&clocks BCM2835_CLOCK_CAM1>;
+			clock-names = "lp";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			#clock-cells = <1>;
+
+			status = "disabled";
+		};
+
 		i2c1: i2c@7e804000 {
 			compatible = "brcm,bcm2835-i2c";
 			reg = <0x7e804000 0x1000>;
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm283x-rpi-csi1-2lane.dtsi
@@ -0,0 +1,7 @@
+&csi1 {
+	port {
+		endpoint {
+			data-lanes = <1 2>;
+		};
+	};
+};
