From 998fa413419cc659e7e8646e63000d77d326e08b Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Thu, 5 Jul 2018 16:44:16 +0100
Subject: [PATCH 342/454] BCM270X_DT: Add CSI defines for all the downstream Pi
 platforms

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2708-rpi-0-w.dts         | 1 +
 arch/arm/boot/dts/bcm2708-rpi-b-plus.dts      | 1 +
 arch/arm/boot/dts/bcm2708-rpi-b.dts           | 1 +
 arch/arm/boot/dts/bcm2708-rpi-cm.dts          | 2 ++
 arch/arm/boot/dts/bcm2709-rpi-2-b.dts         | 1 +
 arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts    | 1 +
 arch/arm/boot/dts/bcm2710-rpi-3-b.dts         | 1 +
 arch/arm/boot/dts/bcm2710-rpi-cm3.dts         | 2 ++
 arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi | 7 +++++++
 arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi | 7 +++++++
 10 files changed, 24 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi
 create mode 100644 arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi

--- a/arch/arm/boot/dts/bcm2708-rpi-0-w.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-0-w.dts
@@ -1,6 +1,7 @@
 /dts-v1/;
 
 #include "bcm2708.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,model-zero-w", "brcm,bcm2835";
--- a/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-b-plus.dts
@@ -2,6 +2,7 @@
 
 #include "bcm2708.dtsi"
 #include "bcm283x-rpi-smsc9514.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	model = "Raspberry Pi Model B+";
--- a/arch/arm/boot/dts/bcm2708-rpi-b.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-b.dts
@@ -2,6 +2,7 @@
 
 #include "bcm2708.dtsi"
 #include "bcm283x-rpi-smsc9512.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	model = "Raspberry Pi Model B";
--- a/arch/arm/boot/dts/bcm2708-rpi-cm.dts
+++ b/arch/arm/boot/dts/bcm2708-rpi-cm.dts
@@ -1,6 +1,8 @@
 /dts-v1/;
 
 #include "bcm2708-rpi-cm.dtsi"
+#include "bcm283x-rpi-csi0-2lane.dtsi"
+#include "bcm283x-rpi-csi1-4lane.dtsi"
 
 / {
 	model = "Raspberry Pi Compute Module";
--- a/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
+++ b/arch/arm/boot/dts/bcm2709-rpi-2-b.dts
@@ -2,6 +2,7 @@
 
 #include "bcm2709.dtsi"
 #include "bcm283x-rpi-smsc9514.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,2-model-b", "brcm,bcm2836";
--- a/arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b-plus.dts
@@ -2,6 +2,7 @@
 
 #include "bcm2710.dtsi"
 #include "bcm283x-rpi-lan7515.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,3-model-b-plus", "brcm,bcm2837";
--- a/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
@@ -2,6 +2,7 @@
 
 #include "bcm2710.dtsi"
 #include "bcm283x-rpi-smsc9514.dtsi"
+#include "bcm283x-rpi-csi1-2lane.dtsi"
 
 / {
 	compatible = "raspberrypi,3-model-b", "brcm,bcm2837";
--- a/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-cm3.dts
@@ -1,6 +1,8 @@
 /dts-v1/;
 
 #include "bcm2710.dtsi"
+#include "bcm283x-rpi-csi0-2lane.dtsi"
+#include "bcm283x-rpi-csi1-4lane.dtsi"
 
 / {
 	model = "Raspberry Pi Compute Module 3";
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-csi0-2lane.dtsi
@@ -0,0 +1,7 @@
+&csi0 {
+	port {
+		endpoint {
+			data-lanes = <1 2>;
+		};
+	};
+};
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x-rpi-csi1-4lane.dtsi
@@ -0,0 +1,7 @@
+&csi1 {
+	port {
+		endpoint {
+			data-lanes = <1 2 3 4>;
+		};
+	};
+};
