From 5d6a82632eb7258c8ca49cc96c18b8b4071b6639 Mon Sep 17 00:00:00 2001
From: Sean Wang <sean.wang@mediatek.com>
Date: Wed, 20 Sep 2017 17:40:16 +0800
Subject: [PATCH 101/224] reset: mediatek: add reset controller dt-bindings
 required header for MT7622 SoC

Add the reset controller dt-bindings exported from infracfg, pericfg,
hifsys and ethsys which could be found on MT7622 SoC. So that we can
reference them from within a device-tree file.

Signed-off-by: Sean Wang <sean.wang@mediatek.com>
Signed-off-by: Philipp Zabel <p.zabel@pengutronix.de>
---
 include/dt-bindings/reset/mt7622-reset.h | 94 ++++++++++++++++++++++++++++++++
 1 file changed, 94 insertions(+)
 create mode 100644 include/dt-bindings/reset/mt7622-reset.h

--- /dev/null
+++ b/include/dt-bindings/reset/mt7622-reset.h
@@ -0,0 +1,94 @@
+/*
+ * Copyright (c) 2017 MediaTek Inc.
+ * Author: Sean Wang <sean.wang@mediatek.com>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+
+#ifndef _DT_BINDINGS_RESET_CONTROLLER_MT7622
+#define _DT_BINDINGS_RESET_CONTROLLER_MT7622
+
+/* INFRACFG resets */
+#define MT7622_INFRA_EMI_REG_RST		0
+#define MT7622_INFRA_DRAMC0_A0_RST		1
+#define MT7622_INFRA_APCIRQ_EINT_RST		3
+#define MT7622_INFRA_APXGPT_RST			4
+#define MT7622_INFRA_SCPSYS_RST			5
+#define MT7622_INFRA_PMIC_WRAP_RST		7
+#define MT7622_INFRA_IRRX_RST			9
+#define MT7622_INFRA_EMI_RST			16
+#define MT7622_INFRA_WED0_RST			17
+#define MT7622_INFRA_DRAMC_RST			18
+#define MT7622_INFRA_CCI_INTF_RST		19
+#define MT7622_INFRA_TRNG_RST			21
+#define MT7622_INFRA_SYSIRQ_RST			22
+#define MT7622_INFRA_WED1_RST			25
+
+/* PERICFG Subsystem resets */
+#define MT7622_PERI_UART0_SW_RST		0
+#define MT7622_PERI_UART1_SW_RST		1
+#define MT7622_PERI_UART2_SW_RST		2
+#define MT7622_PERI_UART3_SW_RST		3
+#define MT7622_PERI_UART4_SW_RST		4
+#define MT7622_PERI_BTIF_SW_RST			6
+#define MT7622_PERI_PWM_SW_RST			8
+#define MT7622_PERI_AUXADC_SW_RST		10
+#define MT7622_PERI_DMA_SW_RST			11
+#define MT7622_PERI_IRTX_SW_RST			13
+#define MT7622_PERI_NFI_SW_RST			14
+#define MT7622_PERI_THERM_SW_RST		16
+#define MT7622_PERI_MSDC0_SW_RST		19
+#define MT7622_PERI_MSDC1_SW_RST		20
+#define MT7622_PERI_I2C0_SW_RST			22
+#define MT7622_PERI_I2C1_SW_RST			23
+#define MT7622_PERI_I2C2_SW_RST			24
+#define MT7622_PERI_SPI0_SW_RST			33
+#define MT7622_PERI_SPI1_SW_RST			34
+#define MT7622_PERI_FLASHIF_SW_RST		36
+
+/* TOPRGU resets */
+#define MT7622_TOPRGU_INFRA_RST			0
+#define MT7622_TOPRGU_ETHDMA_RST		1
+#define MT7622_TOPRGU_DDRPHY_RST		6
+#define MT7622_TOPRGU_INFRA_AO_RST		8
+#define MT7622_TOPRGU_CONN_RST			9
+#define MT7622_TOPRGU_APMIXED_RST		10
+#define MT7622_TOPRGU_CONN_MCU_RST		12
+
+/* PCIe/SATA Subsystem resets */
+#define MT7622_SATA_PHY_REG_RST			12
+#define MT7622_SATA_PHY_SW_RST			13
+#define MT7622_SATA_AXI_BUS_RST			15
+#define MT7622_PCIE1_CORE_RST			19
+#define MT7622_PCIE1_MMIO_RST			20
+#define MT7622_PCIE1_HRST			21
+#define MT7622_PCIE1_USER_RST			22
+#define MT7622_PCIE1_PIPE_RST			23
+#define MT7622_PCIE0_CORE_RST			27
+#define MT7622_PCIE0_MMIO_RST			28
+#define MT7622_PCIE0_HRST			29
+#define MT7622_PCIE0_USER_RST			30
+#define MT7622_PCIE0_PIPE_RST			31
+
+/* SSUSB Subsystem resets */
+#define MT7622_SSUSB_PHY_PWR_RST		3
+#define MT7622_SSUSB_MAC_PWR_RST		4
+
+/* ETHSYS Subsystem resets */
+#define MT7622_ETHSYS_SYS_RST			0
+#define MT7622_ETHSYS_MCM_RST			2
+#define MT7622_ETHSYS_HSDMA_RST			5
+#define MT7622_ETHSYS_FE_RST			6
+#define MT7622_ETHSYS_GMAC_RST			23
+#define MT7622_ETHSYS_EPHY_RST			24
+#define MT7622_ETHSYS_CRYPTO_RST		29
+#define MT7622_ETHSYS_PPE_RST			31
+
+#endif  /* _DT_BINDINGS_RESET_CONTROLLER_MT7622 */
