From bc70c7f1174b937af2784977281a1567f69dd2b6 Mon Sep 17 00:00:00 2001
From: Chaotian Jing <chaotian.jing@mediatek.com>
Date: Mon, 16 Oct 2017 09:46:31 +0800
Subject: [PATCH 152/224] mmc: mediatek: make hs400_tune_response only for
 mt8173

the origin design of hs400_tune_response is for mt8173 because of
mt8173 has a special design. for doing that, we add a new member
"compatible", by now it's only for mt8173.

Signed-off-by: Chaotian Jing <chaotian.jing@mediatek.com>
Tested-by: Sean Wang <sean.wang@mediatek.com>
Signed-off-by: Ulf Hansson <ulf.hansson@linaro.org>
---
 drivers/mmc/host/mtk-sd.c | 11 +++++++++--
 1 file changed, 9 insertions(+), 2 deletions(-)

--- a/drivers/mmc/host/mtk-sd.c
+++ b/drivers/mmc/host/mtk-sd.c
@@ -302,6 +302,7 @@ struct msdc_save_para {
 
 struct mtk_mmc_compatible {
 	u8 clk_div_bits;
+	bool hs400_tune; /* only used for MT8173 */
 };
 
 struct msdc_tune_para {
@@ -362,18 +363,22 @@ struct msdc_host {
 
 static const struct mtk_mmc_compatible mt8135_compat = {
 	.clk_div_bits = 8,
+	.hs400_tune = false,
 };
 
 static const struct mtk_mmc_compatible mt8173_compat = {
 	.clk_div_bits = 8,
+	.hs400_tune = true,
 };
 
 static const struct mtk_mmc_compatible mt2701_compat = {
 	.clk_div_bits = 12,
+	.hs400_tune = false,
 };
 
 static const struct mtk_mmc_compatible mt2712_compat = {
 	.clk_div_bits = 12,
+	.hs400_tune = false,
 };
 
 static const struct of_device_id msdc_of_ids[] = {
@@ -668,7 +673,8 @@ static void msdc_set_mclk(struct msdc_ho
 		       host->base + PAD_CMD_TUNE);
 	}
 
-	if (timing == MMC_TIMING_MMC_HS400)
+	if (timing == MMC_TIMING_MMC_HS400 &&
+	    host->dev_comp->hs400_tune)
 		sdr_set_field(host->base + PAD_CMD_TUNE,
 			      MSDC_PAD_TUNE_CMDRRDLY,
 			      host->hs400_cmd_int_delay);
@@ -1597,7 +1603,8 @@ static int msdc_execute_tuning(struct mm
 	struct msdc_host *host = mmc_priv(mmc);
 	int ret;
 
-	if (host->hs400_mode)
+	if (host->hs400_mode &&
+	    host->dev_comp->hs400_tune)
 		ret = hs400_tune_response(mmc, opcode);
 	else
 		ret = msdc_tune_response(mmc, opcode);
