From 6cec997da72fcd729caeac384421f0419aed3020 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 5 Feb 2018 10:37:54 +0000
Subject: [PATCH 191/454] config: Add SND_USB_HIFACE=m

See: https://github.com/raspberrypi/linux/issues/2368

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/configs/bcm2709_defconfig | 1 +
 arch/arm/configs/bcmrpi_defconfig  | 1 +
 2 files changed, 2 insertions(+)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -864,6 +864,7 @@ CONFIG_SND_USB_UA101=m
 CONFIG_SND_USB_CAIAQ=m
 CONFIG_SND_USB_CAIAQ_INPUT=y
 CONFIG_SND_USB_6FIRE=m
+CONFIG_SND_USB_HIFACE=m
 CONFIG_SND_SOC=m
 CONFIG_SND_BCM2835_SOC_I2S=m
 CONFIG_SND_BCM2708_SOC_GOOGLEVOICEHAT_SOUNDCARD=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -857,6 +857,7 @@ CONFIG_SND_USB_UA101=m
 CONFIG_SND_USB_CAIAQ=m
 CONFIG_SND_USB_CAIAQ_INPUT=y
 CONFIG_SND_USB_6FIRE=m
+CONFIG_SND_USB_HIFACE=m
 CONFIG_SND_SOC=m
 CONFIG_SND_BCM2835_SOC_I2S=m
 CONFIG_SND_BCM2708_SOC_GOOGLEVOICEHAT_SOUNDCARD=m
