/dts-v1/;

#include "ASL26555.dtsi"

/ {
	compatible = "alphanetworks,asl26555-16m", "alphanetworks,asl26555", "ralink,rt3050-soc";
	model = "Alpha ASL26555 (16M)";
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "uboot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xf80000>;
			};

			partition@fd0000 {
				label = "cert";
				reg = <0xfd0000 0x10000>;
				read-only;
			};

			partition@fe0000 {
				label = "langpack";
				reg = <0xfe0000 0x10000>;
				read-only;
			};

			devdata: partition@ff0000 {
				label = "devdata";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};
