// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "xzwifi,creativebox-v1", "mediatek,mt7621-soc";
	model = "CreativeBox v1";

	aliases {
		led-boot = &led_sys;
		led-failsafe = &led_sys;
		led-running = &led_sys;
		led-upgrade = &led_sys;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x1C000000>,
		      <0x20000000 0x4000000>;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	leds {
		compatible = "gpio-leds";

		power {
			label = "creativebox-v1:blue:power";
			gpios = <&gpio0 31 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led_sys: sys {
			label = "creativebox-v1:blue:sys";
			gpios = <&gpio1 0 GPIO_ACTIVE_LOW>;
		};

		internet {
			label = "creativebox-v1:blue:internet";
			gpios = <&gpio0 29 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "creativebox-v1:blue:wlan2g";
			gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "creativebox-v1:blue:wlan5g";
			gpios = <&gpio0 28 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		power_usb2 {
			gpio-export,name = "power_usb2";
			gpio-export,output = <1>;
			gpios = <&gpio0 22 GPIO_ACTIVE_HIGH>;
		};

		power_usb3 {
			gpio-export,name = "power_usb3";
			gpio-export,output = <1>;
			gpios = <&gpio0 25 GPIO_ACTIVE_HIGH>;
		};

		power_sata {
			gpio-export,name = "power_sata";
			gpio-export,output = <1>;
			gpios = <&gpio0 27 GPIO_ACTIVE_HIGH>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x1fb0000>;
			};
		};
	};
};

&sdhci {
	status = "okay";
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "pci1400,7603";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0000>;
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "pci14c3,7662";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&ethernet {
	mtd-mac-address = <&factory 0xe000>;
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "wdt", "rgmii2";
			ralink,function = "gpio";
		};
	};
};
