From 29e154716049310bb8c559f742bf2b460d5b6bbc Mon Sep 17 00:00:00 2001
From: Chaotian Jing <chaotian.jing@mediatek.com>
Date: Mon, 16 Oct 2017 09:46:38 +0800
Subject: [PATCH 159/224] mmc: mediatek: improve eMMC hs400 mode read
 performance

enlarge outstanding value to improve read performance

Signed-off-by: Chaotian Jing <chaotian.jing@mediatek.com>
Tested-by: Sean Wang <sean.wang@mediatek.com>
Signed-off-by: Ulf Hansson <ulf.hansson@linaro.org>
---
 drivers/mmc/host/mtk-sd.c | 9 +++++++++
 1 file changed, 9 insertions(+)

--- a/drivers/mmc/host/mtk-sd.c
+++ b/drivers/mmc/host/mtk-sd.c
@@ -81,6 +81,7 @@
 #define PAD_DS_TUNE      0x188
 #define PAD_CMD_TUNE     0x18c
 #define EMMC50_CFG0      0x208
+#define EMMC50_CFG3      0x220
 #define SDC_FIFO_CFG     0x228
 
 /*--------------------------------------------------------------------------*/
@@ -251,6 +252,8 @@
 #define EMMC50_CFG_CRCSTS_EDGE    (0x1 << 3)   /* RW */
 #define EMMC50_CFG_CFCSTS_SEL     (0x1 << 4)   /* RW */
 
+#define EMMC50_CFG3_OUTS_WR       (0x1f << 0)  /* RW */
+
 #define SDC_FIFO_CFG_WRVALIDSEL   (0x1 << 24)  /* RW */
 #define SDC_FIFO_CFG_RDVALIDSEL   (0x1 << 25)  /* RW */
 
@@ -320,6 +323,7 @@ struct msdc_save_para {
 	u32 pad_ds_tune;
 	u32 pad_cmd_tune;
 	u32 emmc50_cfg0;
+	u32 emmc50_cfg3;
 	u32 sdc_fifo_cfg;
 };
 
@@ -1750,6 +1754,9 @@ static int msdc_prepare_hs400_tuning(str
 	writel(host->hs400_ds_delay, host->base + PAD_DS_TUNE);
 	/* hs400 mode must set it to 0 */
 	sdr_clr_bits(host->base + MSDC_PATCH_BIT2, MSDC_PATCH_BIT2_CFGCRCSTS);
+	/* to improve read performance, set outstanding to 2 */
+	sdr_set_field(host->base + EMMC50_CFG3, EMMC50_CFG3_OUTS_WR, 2);
+
 	return 0;
 }
 
@@ -2000,6 +2007,7 @@ static void msdc_save_reg(struct msdc_ho
 	host->save_para.pad_ds_tune = readl(host->base + PAD_DS_TUNE);
 	host->save_para.pad_cmd_tune = readl(host->base + PAD_CMD_TUNE);
 	host->save_para.emmc50_cfg0 = readl(host->base + EMMC50_CFG0);
+	host->save_para.emmc50_cfg3 = readl(host->base + EMMC50_CFG3);
 	host->save_para.sdc_fifo_cfg = readl(host->base + SDC_FIFO_CFG);
 }
 
@@ -2017,6 +2025,7 @@ static void msdc_restore_reg(struct msdc
 	writel(host->save_para.pad_ds_tune, host->base + PAD_DS_TUNE);
 	writel(host->save_para.pad_cmd_tune, host->base + PAD_CMD_TUNE);
 	writel(host->save_para.emmc50_cfg0, host->base + EMMC50_CFG0);
+	writel(host->save_para.emmc50_cfg3, host->base + EMMC50_CFG3);
 	writel(host->save_para.sdc_fifo_cfg, host->base + SDC_FIFO_CFG);
 }
 
