From b92c017deda819e45a0f054f6df6b53e645d7fe4 Mon Sep 17 00:00:00 2001
From: zhengbin <zhengbin13@huawei.com>
Date: Tue, 24 Dec 2019 22:16:06 +0800
Subject: [PATCH] brcmfmac: use true,false for bool variable

Fixes coccicheck warning:

drivers/net/wireless/broadcom/brcm80211/brcmfmac/fwsignal.c:911:2-24: WARNING: Assignment of 0/1 to bool variable

Reported-by: Hulk Robot <hulkci@huawei.com>
Signed-off-by: zhengbin <zhengbin13@huawei.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/fwsignal.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/fwsignal.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/fwsignal.c
@@ -912,7 +912,7 @@ static u8 brcmf_fws_hdrpush(struct brcmf
 	wlh += wlh[1] + 2;
 
 	if (entry->send_tim_signal) {
-		entry->send_tim_signal = 0;
+		entry->send_tim_signal = false;
 		wlh[0] = BRCMF_FWS_TYPE_PENDING_TRAFFIC_BMP;
 		wlh[1] = BRCMF_FWS_TYPE_PENDING_TRAFFIC_BMP_LEN;
 		wlh[2] = entry->mac_handle;
