From 2635853ce4ab7654a77ab7080fb56de83408606b Mon Sep 17 00:00:00 2001
From: Wright Feng <wright.feng@cypress.com>
Date: Thu, 12 Dec 2019 00:52:51 +0100
Subject: [PATCH 7/7] brcmfmac: not set mbss in vif if firmware does not
 support MBSS

With RSDB mode, FMAC and firmware are able to create 2 or more AP,
so we should not set mbss in vif structure if firmware does not
support MBSS feature.

Signed-off-by: Wright Feng <wright.feng@cypress.com>
Signed-off-by: Soeren Moch <smoch@web.de>
Reviewed-by: Chi-Hsien Lin <chi-hsien.lin@cypress.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.c
@@ -5293,6 +5293,7 @@ struct brcmf_cfg80211_vif *brcmf_alloc_v
 	struct brcmf_cfg80211_vif *vif_walk;
 	struct brcmf_cfg80211_vif *vif;
 	bool mbss;
+	struct brcmf_if *ifp = brcmf_get_ifp(cfg->pub, 0);
 
 	brcmf_dbg(TRACE, "allocating virtual interface (size=%zu)\n",
 		  sizeof(*vif));
@@ -5305,7 +5306,8 @@ struct brcmf_cfg80211_vif *brcmf_alloc_v
 
 	brcmf_init_prof(&vif->profile);
 
-	if (type == NL80211_IFTYPE_AP) {
+	if (type == NL80211_IFTYPE_AP &&
+	    brcmf_feat_is_enabled(ifp, BRCMF_FEAT_MBSS)) {
 		mbss = false;
 		list_for_each_entry(vif_walk, &cfg->vif_list, list) {
 			if (vif_walk->wdev.iftype == NL80211_IFTYPE_AP) {
