From 31a7809e5c35dc488c7ab889481f25cffc8d8c1b Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 21 Mar 2018 13:53:39 +0000
Subject: [PATCH 256/454] overlays: Update 'upstream' overlay with new dwc2

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/upstream-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/upstream-overlay.dts
+++ b/arch/arm/boot/dts/overlays/upstream-overlay.dts
@@ -126,7 +126,7 @@
 			dr_mode = "otg";
 			g-np-tx-fifo-size = <32>;
 			g-rx-fifo-size = <256>;
-			g-tx-fifo-size = <512 512 512 512 512 768>;
+			g-tx-fifo-size = <512 512 512 512 512 256 256>;
 			status = "okay";
 		};
 	};
