From 52499594ce8b48c434bed29062c8bbc15b96cc96 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Wed, 21 Feb 2018 15:39:26 +0000
Subject: [PATCH 400/454] staging: bcm2835-camera: Fix missing lines between
 items

Fix checkpatch errors for missing blank lines after variable
or structure declarations.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 .../staging/vc04_services/bcm2835-camera/bcm2835-camera.h   | 1 +
 drivers/staging/vc04_services/bcm2835-camera/controls.c     | 2 ++
 drivers/staging/vc04_services/bcm2835-camera/mmal-vchiq.c   | 6 ++++--
 3 files changed, 7 insertions(+), 2 deletions(-)

--- a/drivers/staging/vc04_services/bcm2835-camera/bcm2835-camera.h
+++ b/drivers/staging/vc04_services/bcm2835-camera/bcm2835-camera.h
@@ -133,6 +133,7 @@ int set_framerate_params(struct bm2835_m
 		(pix_fmt)->pixelformat, (pix_fmt)->bytesperline,	\
 		(pix_fmt)->sizeimage, (pix_fmt)->colorspace, (pix_fmt)->priv); \
 }
+
 #define v4l2_dump_win_format(level, debug, dev, win_fmt, desc)	\
 {	\
 	v4l2_dbg(level, debug, dev,	\
--- a/drivers/staging/vc04_services/bcm2835-camera/controls.c
+++ b/drivers/staging/vc04_services/bcm2835-camera/controls.c
@@ -56,6 +56,7 @@ static const s64 ev_bias_qmenu[] = {
 static const s64 iso_qmenu[] = {
 	0, 100000, 200000, 400000, 800000,
 };
+
 static const uint32_t iso_values[] = {
 	0, 100, 200, 400, 800,
 };
@@ -1272,6 +1273,7 @@ int bm2835_mmal_init_controls(struct bm2
 				 * mismatches.
 				 */
 				int i;
+
 				mask = 1 << V4L2_SCENE_MODE_NONE;
 				for (i = 0;
 				     i < ARRAY_SIZE(scene_configs);
--- a/drivers/staging/vc04_services/bcm2835-camera/mmal-vchiq.c
+++ b/drivers/staging/vc04_services/bcm2835-camera/mmal-vchiq.c
@@ -1886,10 +1886,12 @@ int vchiq_mmal_finalise(struct vchiq_mma
 
 int vchiq_mmal_init(struct vchiq_mmal_instance **out_instance)
 {
-	int status;
-	struct vchiq_mmal_instance *instance;
 	static VCHI_CONNECTION_T *vchi_connection;
+
 	static VCHI_INSTANCE_T vchi_instance;
+
+	struct vchiq_mmal_instance *instance;
+	int status;
 	SERVICE_CREATION_T params = {
 		.version		= VCHI_VERSION_EX(VC_MMAL_VER, VC_MMAL_MIN_VER),
 		.service_id		= VC_MMAL_SERVER_NAME,
