From acdfcc7ef78c46baca1439a1cac5b73008abc672 Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Tue, 16 May 2017 11:55:58 +0100
Subject: net: mvneta: hack fix phy_interface

Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
---
 drivers/net/ethernet/marvell/mvneta.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -427,6 +427,7 @@ struct mvneta_port {
 	u16 tx_ring_size;
 	u16 rx_ring_size;
 
+	phy_interface_t phy_interface;
 	struct device_node *dn;
 	unsigned int tx_csum_limit;
 	struct phylink *phylink;
@@ -4314,6 +4315,7 @@ static int mvneta_probe(struct platform_
 
 	pp = netdev_priv(dev);
 	spin_lock_init(&pp->lock);
+	pp->phy_interface = phy_mode;
 	pp->dn = dn;
 
 	pp->rxq_def = rxq_def;
