From 2daca52b80afdc92e7c976629a2bf8182335a626 Mon Sep 17 00:00:00 2001
From: Christian Weiske <cweiske@cweiske.de>
Date: Thu, 3 Jan 2019 20:10:14 +0000
Subject: [PATCH 23/32] Fix typo in ra-param man page section.

Signed-off-by: Kevin Darbyshire-Bryant <ldir@darbyshire-bryant.me.uk>
---
 man/dnsmasq.8    | 2 +-
 man/fr/dnsmasq.8 | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/man/dnsmasq.8
+++ b/man/dnsmasq.8
@@ -1829,7 +1829,7 @@ The interval between router advertisemen
 .B --ra-param=eth0,60.
 The lifetime of the route may be changed or set to zero, which allows
 a router to advertise prefixes but not a route via itself. 
-.B --ra-parm=eth0,0,0
+.B --ra-param=eth0,0,0
 (A value of zero for the interval means the default value.) All four parameters may be set at once.
 .B --ra-param=eth0,mtu:1280,low,60,1200
 
--- a/man/fr/dnsmasq.8
+++ b/man/fr/dnsmasq.8
@@ -1774,7 +1774,7 @@ Un intervalle (en secondes) entre les an
 .B --ra-param=eth0,60.
 La durée de vie de la route peut être changée ou mise à zéro, auquel cas
 le routeur peut annoncer les préfixes mais pas de route :
-.B --ra-parm=eth0,0,0
+.B --ra-param=eth0,0,0
 (une valeur de zéro pour l'intervalle signifie qu'il garde la valeur par défaut).
 Ces quatre paramètres peuvent être configurés en une fois :
 .B --ra-param=eth0,mtu:1280,low,60,1200
