From 6ba6a07ab6d7162652246f895c672ed488877eb1 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 15 Feb 2018 16:03:04 +0000
Subject: [PATCH 208/454] overlay: Add missing pinctrl reference to gpio-ir

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/gpio-ir-overlay.dts | 2 ++
 1 file changed, 2 insertions(+)

--- a/arch/arm/boot/dts/overlays/gpio-ir-overlay.dts
+++ b/arch/arm/boot/dts/overlays/gpio-ir-overlay.dts
@@ -10,6 +10,8 @@
                 __overlay__ {
                         gpio_ir: ir-receiver@12 {
                                 compatible = "gpio-ir-receiver";
+                                pinctrl-names = "default";
+                                pinctrl-0 = <&gpio_ir_pins>;
 
                                 // pin number, high or low
                                 gpios = <&gpio 18 1>;
