From 052669bc0d8bba9b93009eedb66c6e9d00a27034 Mon Sep 17 00:00:00 2001
From: Nick Bulleid <nedbulleid@fastmail.com>
Date: Sat, 12 May 2018 20:44:34 +0100
Subject: [PATCH 299/454] Added export feature to gpio-poweroff documentation

Signed-off-by: Nick Bulleid <nedbulleid@fastmail.com>
---
 Documentation/devicetree/bindings/power/reset/gpio-poweroff.txt | 1 +
 1 file changed, 1 insertion(+)

--- a/Documentation/devicetree/bindings/power/reset/gpio-poweroff.txt
+++ b/Documentation/devicetree/bindings/power/reset/gpio-poweroff.txt
@@ -27,6 +27,7 @@ Optional properties:
   it to an output when the power-off handler is called. If this optional
   property is not specified, the GPIO is initialized as an output in its
   inactive state.
+- export : Export the GPIO line to the sysfs system
 
 Examples:
 
