/dts-v1/;

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "gnubee,gb-pc1", "mediatek,mt7621-soc";
	model = "GB-PC1";

	aliases {
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x1c000000>, <0x20000000 0x4000000>;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 18 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		system {
			label = "gb-pc1:green:system";
			gpios = <&gpio0 6 GPIO_ACTIVE_LOW>;
		};

		led_status: status {
			label = "gb-pc1:green:status";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		lan1 {
			label = "gb-pc1:green:lan1";
			gpios = <&gpio0 24 GPIO_ACTIVE_LOW>;
		};

		lan2 {
			label = "gb-pc1:green:lan2";
			gpios = <&gpio0 25 GPIO_ACTIVE_LOW>;
		};
	};
};

&sdhci {
	status = "okay";
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <80000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x1fb0000>;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&factory 0xe000>;
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "jtag", "rgmii2", "uart3", "wdt";
			ralink,function = "gpio";
		};
	};
};
