/dts-v1/;

#include "rt5350.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "intenso,memory2move", "ralink,rt5350-soc";
	model = "Intenso Memory 2 Move";

	aliases {
		led-boot = &led_wifi;
		led-failsafe = &led_wifi;
		led-running = &led_wifi;
		led-upgrade = &led_wifi;
	};

	chosen {
		bootargs = "console=ttyS0,57600n8 root=/dev/mtdblock5";
	};

	leds {
		compatible = "gpio-leds";

		led_wifi: wifi {
			label = "m2m:blue:wifi";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		wan {
			label = "m2m:green:wan";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		power {
			label = "power";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
		};

		reset {
			label = "reset";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "Bootloader";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "Config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "Factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&esw {
	mediatek,portmap = <0x2f>;
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x0>;
};
