From 17681f0bb474d0d227f07369144149d1555d8bce Mon Sep 17 00:00:00 2001
From: Chen Minqiang <ptpt52@gmail.com>
Date: Sun, 17 Jun 2018 04:14:13 +0800
Subject: [PATCH] essedma: alloc skb ip align

Signed-off-by: Chen Minqiang <ptpt52@gmail.com>
---
 drivers/net/ethernet/qualcomm/essedma/edma.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/qualcomm/essedma/edma.c
+++ b/drivers/net/ethernet/qualcomm/essedma/edma.c
@@ -201,7 +201,7 @@ static int edma_alloc_rx_buf(struct edma
 			skb = sw_desc->skb;
 		} else {
 			/* alloc skb */
-			skb = netdev_alloc_skb(edma_netdev[0], length);
+			skb = netdev_alloc_skb_ip_align(edma_netdev[0], length);
 			if (!skb) {
 				/* Better luck next round */
 				break;
